{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":179,"n_cols":11,"rows_kept":179,"merged":[[0,0,0,10],[2,0,42,0],[2,9,42,9],[43,0,83,0],[43,9,83,9],[52,2,53,2],[84,0,129,0],[84,9,129,9],[130,0,136,0],[130,9,136,9],[137,0,142,0],[137,9,142,9],[143,0,155,0],[143,9,155,9],[156,0,158,0],[156,9,158,9],[159,0,171,0],[159,9,171,9],[172,0,176,0],[172,9,176,9],[177,0,177,8],[178,0,181,0],[178,1,181,10]],"flags":["formulas_cached_only"]}
["制水分公司等部门主要仪器仪表维护清单"]
["场站名称","序号","代码","安装位置","设备名称","规格","型号","厂商品牌","数量","小计","计量单位"]
["菜坝水厂",1,"LT601~602","配水井","超声波液位计","一体式，0~10m","SITRANS LU 150","SIEMENS",2,98,"台"]
[null,2,"LDT601~","配水井","超声波液位差计","一体式，0~1m","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",2,null,"台"]
[null,3,"PH/T202","加药间仪表室","原水PH/温度检测仪","0~14,0~60℃","PC1R1A+SC200","HACH",1,null,"台"]
[null,4,"NHN202","加药间仪表室","原水氨氮分析仪","0~1mg/L","AMTAX INTER2","HACH",1,null,"台"]
[null,5,"COD202","加药间仪表室","原水COD分析仪","0~10mg/L","COD-203A(S)","DKK-TOA(HACH)",1,null,"台"]
[null,6,"TU202","加药间仪表室","原水浊度分析仪","0~9999NTU",null,"HACH",1,null,"台"]
[null,7,"FT601~604","进出配水井","取水配水电磁流量计","DN1200,1.0Mpa","OPTIFLUX2050W","KROHNE",4,null,"套"]
[null,8,"TU602~603","预沉池末端","预沉后浊度分析仪","0~3000NTU",null,"HACH",2,null,"套"]
[null,9,"CL601~602","沉淀池前端","前加氯余氯分析仪","0~3mg/L","CL17 Chlorine analgzer","HACH(停用封存)",0,null,"套"]
[null,10,"TU605~606,TU608~609","沉淀池前端","沉淀前浊度分析仪","0~1000NTU",null,"HACH",4,null,"套"]
[null,11,"TU607,TU610","沉淀池末端","沉淀后浊度分析仪","0~100NTU",null,"HACH",2,null,"套"]
[null,12,"SI601~604","沉淀池行车","沉淀池污泥界面仪","一体式，0~5m","SONATAX sc+SC200","HACH",4,null,"套"]
[null,13,"LT401~406,LT407~412","滤池","超声波液位计","一体式，0~5m","SITRANS LU 150 ","SIEMENS",12,null,"套"]
[null,14,"CL401~402","滤池","砂滤后余氯分析仪","0~3mg/L","CL17 Chlorine analgzer","HACH",2,null,"套"]
[null,15,"TU401~402","滤池","砂滤后浊度分析仪","0~5NTU","1720E +SC200","HACH",2,null,"套"]
[null,16,"PT301~307","反冲洗泵房","远传压力表","0~1.0Mpa","SITRANS P DS III","SIEMENS",7,null,"套"]
[null,17,"FT301","反冲洗泵房","空气流量电磁流量计","DN25,1.0Mpa",null,null,1,null,"套"]
[null,18,"LT201~202,LT209~210","吸水井","超声波液位计","一体式，0~10m",null,"SIEMENS",4,null,"套"]
[null,19,"LT203~206","清水池","超声波液位计","一体式，0~10m",null,"SIEMENS",4,null,"套"]
[null,20,"PT201~204","送水泵房","真空压力表","0~1.0Mpa","SITRANS P DS III","SIEMENS",4,null,"套"]
[null,21,"PT205~210","送水泵房","远传压力表","0~1.0Mpa","SITRANS P DS III","SIEMENS",6,null,"套"]
[null,22,"PH/T201","送水泵房","出厂水PH/温度检测仪","0~14,0~60℃","PC1R1A+SC200","HACH",1,null,"台"]
[null,23,"NHN201","送水泵房","出厂水氨氮分析仪","0~1mg/L","AMTAX INTER2","HACH",1,null,"台"]
[null,24,"COD201","送水泵房","出厂水COD分析仪","0~10mg/L","COD-203A(S)","HACH",1,null,"台"]
[null,25,"TU201","送水泵房","出厂水浊度分析仪","0~5NTU","1720E +SC200","HACH",1,null,"台"]
[null,26,"CL201","送水泵房","出厂水余氯分析仪","0~3mg/L","CL17 Chlorine analgzer","HACH",1,null,"套"]
[null,27,"FT201~202","送水泵房出口","送水电磁流量计","DN1200,1.0Mpa","OPTIFLUX2050W","KROHNE",2,null,"套"]
[null,28,"LT503~504","贮泥池","超声波液位计","一体式，0~5m","XRS-5 ULTRASONIC +Multiranger 100","HACH",2,null,"套"]
[null,29,"SS503~504","贮泥池","污泥浓度计","0~20000mg/L",null,"HACH",2,null,"套"]
[null,30,"SS501~502","浓缩池","污泥浓度计","0~20000mg/L",null,"HACH",2,null,"套"]
[null,31,"SI501~502","浓缩池","污泥界面仪","0~5m配套传感器","SONATAX sc+SC200","HACH",2,null,"套"]
[null,32,"LT501~502","排泥池","超声波液位计","一体式，0~7m","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",2,null,"套"]
[null,33,"LT506~507","回收水池","超声波液位计","一体式，0~5m","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",2,null,"套"]
[null,34,"FT507","回收水池","电磁流量计","DN600,PN1.0MPa",null,"渤海",1,null,"套"]
[null,35,"FT508","污泥回流","电磁流量计","DN350,PN1.0MPa",null,"渤海",1,null,"套"]
[null,36,"LT101","取水泵房","静压式液位计","0~30m",null,"HACH",1,null,"套"]
[null,37,"PT101,102,104,105,106","取水泵房","远传压力表","0~1.0MPa","SITRANS P DS III","SIEMENS",5,null,"套"]
[null,38,"PT107,108,110","取水泵房","真空远传压力表","0~1.0Mpa","SITRANS P DS III","SIEMENS",3,null,"套"]
[null,39,null,"加氯间","二氧化氯检测仪",null,"9187sc+SC200","HACH",1,null,"套"]
[null,40,null,"加药间仪表室","氟离子浓度检测仪",null,"FBM-100A","DKK-TOA(HACH)",1,null,"套"]
[null,null,"小计",{"$nulls":5},98]
["普安水厂",1,"PH/T101","原水监测中心","原水PH/温度检测仪","0~14,0~60℃","PC1R1A+SC200","HACH",1,106,"套"]
[null,2,"TU101","原水监测中心","浊度仪","0-4000NTU",null,"HACH",1,null,"套"]
[null,3,"COD101","原水监测中心","COD检测仪","0-100mg/L","COD-203A(S)","DKK-TOA(HACH)",1,null,"套"]
[null,4,"NH3-N101","原水监测中心","氨氮检测仪","0-100mg/L","AMTAX INTER2","HACH",1,null,"套"]
[null,5,"LT201~203","排泥综合池","超声波液位计","0-10M,FMU42","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",3,null,"套"]
[null,6,"LT204-205","贮泥池","超声波液位计","0-5M,FMU40","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",2,null,"套"]
[null,8,"FT201-202","泥渣脱水间","电磁流量计","DN40,IP67",null,null,2,null,"套"]
[null,9,"LDT201~202","配水井","超声波液位差计","0-3m/0-0.5m,FMU90+2*FDU91","XRS-5 ULTRASONIC +Multiranger 200","SIEMENS",2,null,"套"]
[null,10,"LT301~306","溶液池溶解池","超声波液位计","0-3m/FMU40","SITRANS LU 150 ","SIEMENS",6,null,"套"]
[null,11,"FT301~306","PAC投加系统","电磁流量计","DN25，IP67",null,"重庆川仪自动化股份有限公司",4,null,"套"]
[null,12,null,"PAC投加系统","电磁流量计","DN20，IP67",null,"重庆川仪自动化股份有限公司",2,null,"套"]
[null,13,"FT307~310","PAM投加系统","电磁流量计","DN40,IP67",null,"重庆川仪自动化股份有限公司",4,null,"套"]
[null,14,"FT311~312","活性炭投加系统","电磁流量计","DN100，IP67",null,null,2,null,"套"]
[null,15,"LT307~309","贮液池","超声波液位计","0-5M,FMU41","SITRANS LU 150 ",null,3,null,"套"]
[null,16,"FT313~314","原水","电磁流量计","DN1200,IP68","SITRANS FUS080","SIEMENS",2,null,"套"]
[null,17,"FT401","厂平，滤池出水","电磁流量计","DN1800，IP68",null,null,1,null,"套"]
[null,18,"PT401~406","反冲洗泵房","压力变送器","0-0.5MPa，PMP51",null,null,6,null,"套"]
[null,19,"TU401","滤池总出水","浊度仪","0-5NTU",null,null,1,null,"套"]
[null,20,"LT401","滤池","超声波液位计","0-5M,FMU41","SITRANS LU 150 ",null,1,null,"套"]
[null,21,"LT501~504","清水池","静压式液位计","0-5M,FMX21",null,null,4,null,"套"]
[null,22,"CL501~502","清水池","余氯检测 ","0-2mg/L","CL17 Chlorine analgzer",null,2,null,"套"]
[null,23,"LT501~503","送水泵房","超声波液位计","0-10M,FMU42","SITRANS LU 150 ",null,3,null,"套"]
[null,24,"FT501~502","出水流量计井","电磁流量计","DN1200,IP68","SITRANS FUS080",null,2,null,"套"]
[null,25,"PT501~508","送水泵房","压力变送器","0-1.0MpA,PMP51","SITRANS P DS III",null,8,null,"套"]
[null,26,"LT601~604","消毒间","超声波液位计","0-5M,FMU40","SITRANS LU 150 ",null,4,null,"套"]
[null,27,"FT601~602","消毒间","电磁流量计","DN15，IP67",null,"重庆川仪自动化股份有限公司",2,null,"套"]
[null,28,"FT603","消毒间","电磁流量计","DN25，IP67",null,"重庆川仪自动化股份有限公司",1,null,"套"]
[null,29,"CLA601","消毒间","漏氯报警仪","GDC-02-AC-AL-LGX",null,null,1,null,"套"]
[null,30,null,"消毒间","漏氯报警探头","0-50ppm，SDT0300",null,null,2,null,"套"]
[null,31,"LT2A01","高效浓缩池","超声波液位计","0-7M,FMU41","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",1,null,"套"]
[null,32,"SS2A01~02","高效浓缩池","污泥浓度计","5-50mg/L",null,null,2,null,"套"]
[null,33,"LT3A01","预沉池","超声波液位计","0-5M,FMU41","XRS-5 ULTRASONIC +Multiranger 100","SIEMENS",2,null,"套"]
[null,34,"TU3A01","预沉池","浊度计","0-500NTU",null,null,2,null,"套"]
[null,35,"FT3A01","预沉池","电磁流量计","DN1200,IP68",null,null,2,null,"套"]
[null,36,"LT3C01~02","沉淀池","超声波液位计","0-5M,FMU41","SITRANS LU 150 ","SIEMENS",4,null,"套"]
[null,37,"TU3C01~02","沉淀池","浊度计","0-500NTU",null,null,4,null,"套"]
[null,38,"LT4A01","单格滤池","超声波液位计","0-5M,FMU41","SITRANS LU 150 ","SIEMENS",12,null,"套"]
[null,39,"TU501","送水泵房","浊度计","0-5NTU","1720E +SC200",null,1,null,"套"]
[null,40,"PH/T501","送水泵房","出厂水PH/温度检测仪","2-12/0-50C","PC1R1A+SC200",null,1,null,"套"]
[null,41,"CL503","送水泵房","余氯检测仪","0-5mg/L","CL17 Chlorine analgzer",null,1,null,"套"]
[null,null,"小计",{"$nulls":5},106]
["五水厂",1,"FT101","五水厂起水原水管","电磁流量计",null,"FST030","SIEMENS（西门子）",1,57,"台"]
[null,2,"FT102","南溪水厂起水原水管","电磁流量计",null,"KSDLDG-DN1400FF1700A2","成都市凯思达机电有限责任公司",1,null,"台"]
[null,3,"PT101","起水1号泵","压力传感器",null,"7MF1567-3CB00-1AAA","SIMENS(西门子）",1,null,"个"]
[null,4,"PT102","起水2号泵","压力传感器",null,"7MF1567-3CB00-1AAA","SIMENS(西门子）",1,null,"个"]
[null,5,"PT103","起水3号泵","压力传感器",null,"7MF1567-3CB00-1AAA","SIMENS(西门子）",1,null,"个"]
[null,6,"PT104","起水4号泵","压力传感器",null,"7MF1567-3CB00-1AAA","SIMENS(西门子）",1,null,"个"]
[null,7,"PT105","五厂起水主管","压力传感器",null,"7MF1567-3CB00-1AAA","SIMENS(西门子）",1,null,"个"]
[null,8,"PT106","南溪起水主管","压力传感器",null,"7MF1567-3CB00-1AAA","SIMENS(西门子）",1,null,"个"]
[null,9,"LT101","起水集水井","液位计",null,"FMU30-AAHEABGHF","Prosonic T",1,null,"套"]
[null,10,"AIW27","送水1号泵","压力变送器",null,"7MF4033-1DA00-2AB6-Z","SIMENS(西门子）",1,null,"套"]
[null,11,"AIW28","送水2号泵","压力变送器",null,"7MF4033-1DA00-2AB6-Z","SIMENS(西门子）",1,null,"套"]
[null,12,"AIW29","送水3号泵","压力变送器",null,"7MF4033-1DA00-2AB6-Z","SIMENS(西门子）",1,null,"套"]
[null,13,"AIW5","送水出水在线","余氯检测仪",null,"YZ60-B","HYteehnology",1,null,"套"]
[null,14,"AIW2/AIW3","送水出水在线","PH+温度计",null,"CM442-3PQ7/0","Endress+Hauser",1,null,"套"]
[null,15,"AIW4","送水出水在线","浊度仪",null,"AV88AQT1AC","Thermo ",1,null,"套"]
[null,16,"AW16","加氯加药间","原药剂电磁流量计1",null,"DJLD-DN50(1-30立方/时）","青岛布莱迪仪表有限公司",1,null,"套"]
[null,17,"AW17","加氯加药间","原药剂电磁流量计2",null,"DJLD-DN50(1-30立方/时）","青岛布莱迪仪表有限公司",1,null,"套"]
[null,18,"AW11","加氯加药间","PAC液位1",null,"FMU30-AAHEABGHF","Prosonic T",1,null,"套"]
[null,19,"AW12","加氯加药间","PAC液位2",null,"FMU30-AAHEABGHF","Prosonic T",1,null,"套"]
[null,20,"AW13","加氯加药间","PAC液位3",null,"FMU30-AAHEABGHF","Prosonic T",1,null,"套"]
[null,21,null,"加氯加药间","PAC稀释流量计1",null,"DJLD-DN25(0.3-10立方/时）","青岛布莱迪仪表有限公司",1,null,"套"]
[null,22,null,"加氯加药间","PAC稀释流量计2",null,"DJLD-DN25(0.3-10立方/时）","青岛布莱迪仪表有限公司",1,null,"套"]
[null,23,null,"加氯加药间","PAM用量1",null,"DJLD-DN25(0.3-10立方/时）","青岛布莱迪仪表有限公司",1,null,"套"]
[null,24,null,"加氯加药间","PAM用量2",null,"DJLD-DN25(0.3-10立方/时）","青岛布莱迪仪表有限公司",1,null,"套"]
[null,25,"AW13、14","泥水调节池","液位计",null,"FMU30-AAHEABGHF","Prosonic T",2,null,"套"]
[null,26,"AW11、12","泥水调节池","电磁流量计转换器",null,"MGG/KL-1231412EC1","开封开流仪表有限公司",2,null,"台"]
[null,27,"AW17、18","浓缩池","浊度仪",null,"AV38BB0A2 ","Thermo ",2,null,"套"]
[null,28,"AW15、16","浓缩池","液位计",null,"FMU30-AAHEABGHF","Prosonic T",2,null,"套"]
[null,29,null,"主体原水管","电磁流量计转换器",null,"MGG/KL-1231412EC1","开封开流仪表有限公司",1,null,"台"]
[null,30,"AIW6","回收水池","电磁流量计转换器",null,"MGG/KL-1231412EC1","开封开流仪表有限公司",1,null,"台"]
[null,31,"AIW7、8","回收水池","液位计",null,"FMU30-AAHEABGHF","Prosonic T",2,null,"套"]
[null,32,null,"一体化设备","电磁流量转换器",null,"LDZ-6-10-10","上海光华仪表有限公司",1,null,"台"]
[null,33,"AIW13","滤池","浊度仪",null,"AV88AQT1AC","Thermo ",1,null,"套"]
[null,34,"AIW9、10、11、12","滤池","液位计",null,"FMU30-AAHEABGHF","Prosonic T",4,null,"套"]
[null,35,"AIW24、25","沉淀池","浊度仪",null,"AV38BB0A2 ","Thermo ",2,null,"套"]
[null,36,"AIW22、23","预沉淀池","浊度仪",null,"AV38BB0A2 ","Thermo ",2,null,"套"]
[null,37,"AIW21","原水预沉淀池","浊度仪",null,"AV38BB0A2 ","Thermo ",1,null,"套"]
[null,38,"AIW19、20","原水预沉淀池","PH+温度计",null,"CM442-3PQ7/0","Endress+Hauser",1,null,"套"]
[null,39,"AIW14、15","清水池","液位计",null,"FMU30-AAHEABGHF","Prosonic T",2,null,"套"]
[null,40,"AIW16、17","吸水井","液位计",null,"FMU30-AAHEABGHF","Prosonic T",2,null,"套"]
[null,41,"AIW18","反冲洗吸水井","液位计",null,"FMU30-AAHEABGHF","Prosonic T",1,null,"套"]
[null,42,"AIW0","送水管1","电磁流量计转换器",null,"MGG/KL-2521412EC1","开封开流仪表有限公司",1,null,"套"]
[null,43,null,"送水管2","电磁流量计",null,"91WA1-AA3C00ACA4AA","Endress+Hauser",1,null,"套"]
[null,44,"AIW1","自给水管1","电磁流量计转换器",null,"MGG/KL-1421412EC1","开封开流仪表有限公司",1,null,"套"]
[null,45,null,"自给水管2","电磁流量计转换器",null,"MGG/KL-1421412EC1","开封开流仪表有限公司",1,null,"套"]
[null,null,"小计",{"$nulls":5},57]
["一水厂",1,null,null,"流量计",{"$nulls":3},3,11,"台"]
[null,2,null,null,"液位计",{"$nulls":3},1,null,"台"]
[null,3,null,null,"PH计",null,null,"哈希",1,null,"台"]
[null,4,null,null,"浊度仪",null,null,"哈希",4,null,"台"]
[null,5,null,null,"二氧化氯",null,null,"哈希",1,null,"台"]
[null,6,null,null,"氨氮在线监测",{"$nulls":3},1,null,"台"]
[null,null,"小计",{"$nulls":5},11]
["二水厂",1,null,"送水车间","流量计",{"$nulls":3},3,28,"台"]
[null,2,null,"制水车间","液位计",{"$nulls":3},20,null,"台"]
[null,3,null,null,"PH计",null,null,"哈希",1,null,"台"]
[null,4,null,null,"浊度仪",null,null,"哈希",3,null,"台"]
[null,5,null,null,"二氧化氯",null,null,"哈希",1,null,"台"]
[null,null,"小计",{"$nulls":5},28]
["四水厂",1,null,"取水泵房","浊度仪",{"$nulls":3},1,20,"只"]
[null,2,null,"取水泵房","PH计",{"$nulls":3},1,null,"只"]
[null,3,null,"取水泵房","电磁流量计","DN800",null,"上海光华",2,null,"只"]
[null,4,null,"送水泵房","电磁流量计","DN800",null,"上海光华",2,null,"只"]
[null,5,null,"清水池","液位计",null,null,"E+H",2,null,"只"]
[null,6,null,"清水池","液位计",null,null,"E+H",2,null,"只"]
[null,7,null,"送水泵房","浊度仪",{"$nulls":3},1,null,"只"]
[null,8,null,"送水泵房","PH计",{"$nulls":3},1,null,"只"]
[null,9,null,"送水泵房","余氯仪",{"$nulls":3},1,null,"只"]
[null,10,null,"滤池","浊度仪",{"$nulls":3},4,null,"只"]
[null,11,null,"滤池","PH计",{"$nulls":3},2,null,"只"]
[null,12,null,"滤池","余氯仪",{"$nulls":3},1,null,"只"]
[null,null,"小计",{"$nulls":5},20]
["管网部",1,null,"岷江新区泵站","流量计",{"$nulls":3},1,2,"套"]
[null,2,null,"岷江新区泵站","液位计",{"$nulls":3},1,null,"套"]
[null,null,"小计",{"$nulls":5},2]
["天泉公司",1,null,"二级泵站","智能数字显示报警仪",null,"WP-C701-02-HL-PASC","上海望源 ",5,19,"套"]
[null,2,null,"高捷水厂","出厂水氯余氯分析仪","0~3mg/L","CL17 Chlorine analgzer+sc200","HACH",1,null,"套"]
[null,3,null,"高捷水厂","出厂水浊度分析仪","0~5NTU","1720E +SC200","HACH",1,null,"套"]
[null,4,null,"高捷水厂","出厂水PH分析仪",null,"9187sc+SC200","HACH",1,null,"套"]
[null,5,null,"高捷水厂清水池","超声波液位计","0~10m","SITRANS Probe lu","SITRANS",1,null,"套"]
[null,6,null,"高捷水厂清水池","超声波液位计","（0-10m）","TS-L300N","浙江东仪科技有限公司",2]
[null,7,null,"高捷水厂清水池","余氯检测仪","（0-20mg/L）","LH-G8210","浙江陆恒环境科技有限公司",2]
[null,8,null,"华嘴水厂","出厂水氯余氯分析仪","0~3mg/L","CL17 Chlorine analgzer+sc200","HACH",1,null,"套"]
[null,9,null,"华嘴水厂","出厂水浊度分析仪","0~5NTU","1720E +SC200","HACH",1,null,"套"]
[null,10,null,"华嘴水厂","智能数字显示报警仪",null,"WP-C701-02-HL-PASC","上海望源 ",1,null,"套"]
[null,11,null,"三级泵站","出厂水氯余氯分析仪","0~3mg/L","CL17 Chlorine analgzer+sc200","HACH",1,null,"套"]
[null,12,null,"三级泵站","智能数字显示报警仪",null,"WP-C701-02-HL-PASC","上海望源 ",2,null,"套"]
[null,null,"小计",{"$nulls":5},19]
["临港公司",1,null,"白沙泵站","余氯监测仪",null,"CL17","HACH",1,8,"套"]
[null,2,null,"白沙泵站","浊度仪",null,"sc200","HACH",1,null,"套"]
[null,3,null,"白沙泵站","流量计",{"$nulls":3},2,null,"台"]
[null,4,null,"白沙泵站","投入式液位计",{"$nulls":3},4,null,"台"]
[null,null,"小计",{"$nulls":5},8,null,"台"]
["合计",{"$nulls":8},349]
["备注"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}